This is a modified version of the opensource mp3 prx for irshell. It will play 
mp3 files from ms0:/PSP/MUSIC . It has random and sequential play modes,
pause, next and a builtin "overclocker".

Copy Install and PSP folders to the root of your memory stick.
Then run UMFR2 For GAME mode and/or UMFR2 For VSH(XMB) mode depending on where you 
want the module to be loaded.

I have only tested this with 2.71 SEB'' with no custom gameboots/backgrounds/other prxs/etc.
These things may reduce compatibility or prevent it from working properly.

It is also a good idea to wait until the game is finished loading up before starting playback.

Controls:
(The Note button is to the left of select)
Note + Left Trigger = pause/resume playback
Note + Right Trigger = switch playback mode between random and seqeuntial
Note + D-Pad Left  = previous song (only in sequential mode)
Note + D-Pad Right  = next song
Note + Triangle = Change CPU speed
Note + Square = Toggle On Screen Display (default off)
Note + Circle = Reload list of mp3 files (needed if you change the files in the music folder using usb)
(when READY is displayed in the bottom left hand corner, press Note+ Left Trigger to start playback)
Note + Cross = Change brightness level (from current up to maximum
Changelog:
0.1: Initial release
0.2: Fixed usb,suspend and resume bugs
     Added a seperate flasher for vsh mode
0.2b: Fixed a bug which could crash the psp if the mp3 filename was too long (Note there is still a limit of 100 mp3 files)
      Added subdirectory scanning (there can be any number of subdirectories)
      Added previous mode in Sequential mode 
      Modified the controls
0.2c: Fixed a bug that would cause a crash if there were more than the max # of mp3s on the memorystick
      Raised the playlist limit to 300 files
      Made on screen display off by default because it sometimes causes a crash 
      Moved allocation of playlist to user mem. This may increase compatibility.
0.3:  Re-did the playlist code so no memory allocation is needed. This saves alot of mem and will reduce crashes.
      Reset to default CPU speed on exit
0.3a: Added more CPU speeds
      Added a brightness toggle including maximum brightness(the one that normally requires your psp to be plugged in) (NOTE+X)            
Uses blitting code from the vshex module in the devhook 043sdk.
-----------------------------------------------------------------------
from orginal irsmp3.prx by AhMan
This MP3 Player plugin is based on the MP3 player from neogeoCD 0.91
from Yoyofr & ZeLurker and is released under the terms of the GUN
General Public License (GPL).  The original MP3 player from neogeoCD
is based on MAD (libmad) MPEG audio decoder library.

To compile this MP3 player, you'll need to download the neogeoCD 0.91
soruce code from http://www.rainemu.com/html/archive/tux/neocdpsp.html.  
After download and extracted the source codes, you'll need to remove
serveral "assert" statements (remove them or comment them out) from
timer.c & layer3.c from the libmad library source.
Then, compile neogeoCD and a libmad.a library will be generated.

To compile the MP3 player, modify the Makefile to point to the newly
generated libmad.a library & header file, or copy them to your MP3 player
source directory.

Cheers,
AhMan
-----------------------------------------------------------------------
//You probably won't need this
The precompiled libmad.a is included along with the source under neocdpspsrc/src/libmad.
To recompile it:
cd neocdpspsrc/src/libmad
./configure
cd ../..
make obj/libmad.a
